# Physical

Network Analysis Module (NAM) Card > Configure

This dialog box displays the following information:

- Name (moduleName)

- Module Model (moduleModel)

- Serial Number (moduleSerialNumber)

- Hardware Version (moduleHwVersion)

- Firmware Version (moduleFwVersion)

- Software Version (moduleSwVersion)

- Status (moduleStatus)

- IP Address (moduleIPAddress)

- Diagnostic Errors (moduleTestResult)

- Intake Temperature (entSensorValue)

- Exhaust Temperature (entSensorValue)

- Device1 Temperature (entSensorValue)

- Device2 Temperature (entSensorValue)

Name (moduleName)

Name assigned to the module or card by the network administrator, such as “London.”

Module Model (moduleModel)

Manufacturer’s model number for the card or module.

Serial Number (moduleSerialNumber)

Serial number of the card or module (for example, 900000023).

Hardware Version (moduleHwVersion)

Version number of the card being managed (for example, 3.1).

Firmware Version (moduleFwVersion)

Firmware version of the card being managed (for example, 2.0).

Software Version (moduleSwVersion)

Software version of the card being managed (for example, 3.2).

Status (moduleStatus)

Current status of the module or card. Possible values are ok, minorFault, majorFault, or other. If the status is not ok, the value of the Diagnostic Errors field gives more information about the cause of the problem.

IP Address (moduleIPAddress)

IP address of the module or card.

Note: This field is only displayed on NAM and IDS modules.

Diagnostic Errors (moduleTestResult)

Result of the module’s self-test. None indicates that the module passed all tests.

Intake Temperature (entSensorValue)

Temperature recorded by the device's intake sensor.

Exhaust Temperature (entSensorValue)

Temperature recorded by the device's exhaust sensor.

Device1 Temperature (entSensorValue)

Temperature recorded by the device1 sensor.

Device2 Temperature (entSensorValue)

Temperature recorded by the device2 sensor.