# AAL5 VCC Traffic

The ATM Adaptation Layer type 5 Virtual Circuit Connections (AAL5 VCC) Traffic dialog box displays AAL5 VCC Traffic for the selected sub interfaces; VPI , VCI values.

## Procedure

1. Right-click the port, then select Monitor.

2. Select AAL5 VCC Performance from the Category list.

3. Select a row and click Monitor. The AAL5 VCC Performance dialog box is displayed.

4. Select AAL5 VCC Traffic from the Category list.

> The following details are displayed.

> PDUs Received (cAal5VccInPkts)

> PDUs Transmitted (cAal5VccOutPkts)

> PDU Octets Received (cAal5VccInOctets)

> PDU Octets Transmitted (cAal5VccOutOctets)

### PDUs Received (cAal5VccInPkts)

The number of ATM Adaptation Layer5 CPCS PDUs received on the AAL5 VCC at the interface associated with an AAL5 entity.

### PDUs Transmitted (cAal5VccOutPkts)

The number of ATM Adaptation Layer5 CPCS PDUs transmitted on the AAL5 VCC at the interface associated with an AAL5 entity.

### PDU Octets Received (cAal5VccInOctets)

The number of AAL5 CPCS PDU octets received on the AAL5 VCC at the interface associated with an AAL5 entity.

### PDU Octets Transmitted (cAal5VccOutOctets)

The number of AAL5 CPCS PDU octets transmitted on the AAL5 VCC at the interface associated with an AAL5 entity.