# Fast Serial Port Configuration Information

The following information is displayed for a fast serial port:

Type

RTS Signal

CTS Signal

DTR Signal

DCD Signal

DSR Signal

# Type (locIfFSIPtype)

Indicates whether the FSIP line uses DCE (data communications equipment) or DTE (data terminal equipment).

# RTS Signal (locIfFSIPrts)

Indicates whether the RTS (Request To Send) signal is up or down. Possible values are up, down, or not available.

# CTS Signal (locIfFSIPcts)

Indicates whether the CTS (Clear To Send) signal is up or down. Possible values are up, down, or not available.

# DTR Signal (locIfFSIPdtr)

Indicates whether the DTR (data terminal ready) signal is up or down. Possible values are up, down, or not available.

# DCD Signal (locIfFSIPdcd)

Indicates whether the DCD (data carrier detect) signal is up or down. Possible values are up, down, or not available.

# DSR Signal (locIfFSIPdsr)

Indicates whether the DSR (data set ready) field is up or down. Possible values are up, down, or not available.