# Mobile Router Registration Configs

1. Right-click on the MWAM Card and select Configure.

2. Select category MWAM module.

3. Select a row and click the Configure button.

4. Select category Mobile Router Registration Configs.

The following information appears:

> Time before Lifetime Expiration (cmiMrRegExtendExpire)

> Number of Retries (cmiMrRegExtendRetry)

> Waiting Time for Reply (cmiMrRegExtendInterval)

> Requested Registration Time (cmiMrRegLifetime)

> Initial Retransmission (cmiMrRegRetransInitial)

> Maximum Retransmission Time (cmiMrRegRetransMax)

> Maxi Retransmissions (cmiMrRegRetransLimit)

### Time before Lifetime Expiration (cmiMrRegExtendExpire)

Time remaining in seconds to send registration request before lifetime expiration.

### Number of Retries (cmiMrRegExtendRetry)

Number of retries to be sent.

### Waiting Time for Reply (cmiMrRegExtendInterval)

Time in seconds after which the mobile router is to send another registration request when no reply is received.

### Requested Registration Time (cmiMrRegLifetime)

Requested lifetime in seconds in registration requests.

### Initial Retransmission (cmiMrRegRetransInitial)

Time in milliseconds to wait after no reply is received before retransmitting for the first time.

### Maximum Retransmission Time (cmiMrRegRetransMax)

Maximum retransmission time allowed (milliseconds).

### Max Retransmission (cmiMrRegRetransLimit)

Maximum number of retransmissions allowed.