# Comparative Charts (DELTA) - STRIP

## Navigation

1. Right-click the Content Switching Module (CSM) and then select Monitor > Fault Tolerance.

2. Select Comparative Charts (DELTA) - STRIP.

The following information is displayed:

> Keep-Alives Received (cslbxFtRxHeartBeatMsgs)

> Keep-Alives Transmitted (cslbxFtTxHeartBeatMsgs)

> State Updates Received (cslbxFtRxUpdateMsgs)

> State Updates Transmitted (cslbxFtTxUpdateMsgs)

> Master Overrides Received (cslbxFtRxCoupMsgs)

> Master Overrides Transmitted (cslbxFtTxCoupMsgs)

> Master Elects Received (cslbxFtRxElectMsgs)

> Master Elects Transmitted (cslbxFtTxElectMsgs)

> Connection Replication Received (cslbxFtRxConnReplMsgs)

> Connection Replications Transitted (cslbxFtTxConnReplMsgs)

> Total FT Packets Received (cslbxFtRxPackets)

> Total FT Packets Dropped (cslbxFtDropPackets)

> Duplicate FT Packets Received (cslbxFtDuplPackets)

> Checksum Error Packets Received (cslbxFtXsumErrPackets)

> Buffer Packets Received (cslbxFtBuffErrPackets)

##

### Keep-Alives Received (cslbxFtRxHeartBeatMsgs)

Number of keep-alive messages received by this Server Load Balancing (SLB) device.

### Keep-Alives Transmitted (cslbxFtTxHeartBeatMsgs)

Number of keep-alive messages sent by this SLB device.

### State Updates Received (cslbxFtRxUpdateMsgs)

Number of state update (sticky) messages received by this SLB device.

### State Updates Transmitted (cslbxFtTxUpdateMsgs)

Number of state update (sticky) messages sent by this SLB device.

### Master Overrides Received (cslbxFtRxCoupMsgs)

Number of master override messages received by this SLB device.

### Master Overrides Transmitted (cslbxFtTxCoupMsgs)

Number of master override messages sent by this SLB device.

### Master Elects Received (cslbxFtRxElectMsgs)

Number of master election messages received by this SLB device.

### Master Elects Transmitted (cslbxFtTxElectMsgs)

Number of master election messages sent by this SLB device.

### Connection Replication Received (cslbxFtRxConnReplMsgs)

Number of connection replication messages received by this SLB device.

### Connection Replications Transitted (cslbxFtTxConnReplMsgs)

Number of connection replication messages sent by this SLB device.

### Total FT Packets Received (cslbxFtRxPackets)

Total number of Fault Tolerance messages received by this Server Load Balancing (SLB) device.

### Total FT Packets Dropped (cslbxFtDropPackets)

Total number of Fault Tolerance messages dropped by this SLB device.

### Duplicate FT Packets Received (cslbxFtDuplPackets)

Total number of duplicate Fault Tolerance messages received by this SLB device.

### Checksum Error Packets Received (cslbxFtXsumErrPackets)

Total number of Fault Tolerance messages with a checksum error received by this SLB device.

### Buffer Packets Received (cslbxFtBuffErrPackets)

Total number of Fault Tolerance messages dropped by this SLB device due to insufficient buffer memory.