# VPDN Failure History

Use this option to view failure records that are referenced with a user name.

## Procedure

To access VPDN Failure History:

1. Right-click the device and select Configure from the popup menu.

> > The Configure Device dialog box appears.

2. Select VPDN Failure History from the Category menu.

The VPDN Failure History dialog box displays:

User Name (cvpdnUnameToFailHistUname)

Tunnel Id (cvpdnUnameToFailHistTunnelId)

User Id (cvpdnUnameToFailHistUserId)

Local Initiated Connection (cvpdnUnameToFailHistLocalInitConn)

Local Name (cvpdnUnameToFailHistLocalName)

Remote Name (cvpdnUnameToFailHistRemoteName)

Source IP Address (cvpdnUnameToFailHistSourceIp)

Destination IP Address (cvpdnUnameToFailHistDestIp)

Failure Count (cvpdnUnameToFailHistCount)

Failure Time (cvpdnUnameToFailHistFailTime)

Failure Type (cvpdnUnameToFailHistFailType)

Failure Reason (cvpdnUnameToFailHistFailReason)

Note : You can view VPDN system information, VPDN tunnel information and VPDN session information only if active tunnels are available.

## Related Topics

VPDN System Information

VPDN Tunnels

VPDN Sessions

User Name (cvpdnUnameToFailHistUname)

The user-name for a failure entry.

Tunnel Id (cvpdnUnameToFailHistTunnelId)

The tunnel ID for a failure entry. If it is the tunnel instigator, the ID is the HGW/LNS tunnel ID; otherwise it is the NAS/LAC tunnel ID.

User Id (cvpdnUnameToFailHistUserId)

The user ID of the failure entry.

Local Initiated Connection (cvpdnUnameToFailHistLocalInitConn)

Indicates whether the tunnel in which the failure occurred was generated locally.

Local Name (cvpdnUnameToFailHistLocalName)

The name of the local VPDN tunnel in which the failure occurred.

It is the NAS/LAC name of the tunnel if the router served is an NAS/LAC or the HGW/LNS name of the tunnel if the system served as the home gateway. The local name is the configured host-name of the router. This object is empty if the failure occurred before successful tunnel projection; thus, no source name will be available.

Remote Name (cvpdnUnameToFailHistRemoteName)

The remote name of the VPDN tunnel in which the failure occurred.

It is the home gateway name of the tunnel if the system is an NAS/LAC or the NAS/LAC name of the tunnel if the system serves as the home gateway. This object is empty if the failure occurred before successful tunnel projection; thus, no source name is available.

Source IP Address (cvpdnUnameToFailHistSourceIp)

The source tunnel IP address in which the failure occurred. It is that of the interface at the instigator end of the tunnel.

Destination IP Address (cvpdnUnameToFailHistDestIp)

The destination tunnel IP address in which the failure occurred. It is that of the interface at the receiver end of the tunnel.

Failure Count (cvpdnUnameToFailHistCount)

This object is incremented when multiple failures have occurred.

A delta >1 indicates that the current failure record is the latest of a series of failures that have been recorded.

Failure Time (cvpdnUnameToFailHistFailTime)

Specifies the time the failure occurred.

Failure Type (cvpdnUnameToFailHistFailType)

The type of failure for the current failure record. An ASCII string form that describes the type of failure for the failure record.

Failure Reason (cvpdnUnameToFailHistFailReason)

The reason for the failure of the current failure record.