# GGSN Virtual Server Table

## Navigation

1. Right-click the device, and select Configure. The Device Configuration dialog box appears.

2. Select GGSN Virtual Server Table from the Category list.

The following information appears:

> Virtual Server Address Type (cGgsnSlbVserAddrType)

> Virtual Server Address (cGgsnSlbVserAddress)

> Next Hop Virtual Server Address Type (cGgsnSlbVserNextHopAddrType)

> Next Hop Virtual Server Address (cGgsnSlbVserNextHopAddress)

> VRF Name (cGgsnSlbVserVrfName)

> Virtual Server Row Status (cGgsnSlbVserRowStatus)

### Virtual Server Address Type (cGgsnSlbVserAddrType)

The address type of the vserver. Only IPv4 IP address type is supported.

### Virtual Server Address (cGgsnSlbVserAddress)

The address of GTP vservers; required only in directed mode. If SLB is running in directed mode and this object is not configured, then the feature remains disabled.

If SLB is running in the dispatched mode, the vserver that forwarded the create request is known to the GGSN and thus it is possible to send the notification directly to the vserver.

### Next Hop Virtual Server Address Type (cGgsnSlbVserNextHopAddrType)

The IP address type to reach the virtual server. Only IPv4 IP address type is supported.

### Next Hop Virtual Server Address (cGgsnSlbVserNextHopAddress)

The IP address to reach the vserver.

### VRF Name (cGgsnSlbVserVrfName)

The VRF name -- on an interface on GGSN that is connected to SLB -- to reach the vserver.

### Virtual Server Row Status (cGgsnSlbVserRowStatus)

Creates a new row in the table or deletes the existing row.