# PPPoE VCL Sessions

The PPPoE VCL (Virtual Circuit Link) Sessions dialog box provides details about the established PPPoE VCL sessions for an interface.

## Procedure

1. Right-click the device, then select PPPoE.

2. Select a row from VCL Session Info Table, then click VCL Sessions.

3. Choose the required VCL to view the session details.

The following information appears:

> Active Sessions (cPppoeVcCurrSessions)

> High Water Mark Established (cPppoeVcHighWaterSessions)

> Maximum Allowed Sessions (cPppoeVcMaxAllowedSessions)

> Threshold Value (cPppoeVcThresholdSessions)

### Active Sessions (cPppoeVcCurrSessions)

The current number of active PPPoE sessions on the VCL.

### High Water Mark Established (cPppoeVcHighWaterSessions)

The high water mark of the established PPPoE sessions on the VCL.

### Maximum Allowed Sessions (cPppoeVcMaxAllowedSessions)

The maximum number of allowed PPPoE sessions on the VCL.

### Threshold Value (cPppoeVcThresholdSessions)

The threshold value of the established PPPoE sessions on the VCL. Default is equal to cPppoeVcMaxAllowedSessions.

###