# SRP Error Statistics

Use this option to monitor error statistics of an interface side with a specific interval number.

## Procedure

To access SRP error statistics information:

1. Right-click the port and select SRP Interface Statistics from the popup menu.

Error Statistics dialog box appears.

2. Select Error Statistics from the Category menu to display SRP error statistics information.

SRP Error Statistics dialog box displays:

Interface Side (srpErrorsIntervalInterfaceSide)

Interface Number (srpErrorsIntervalNumber)

### Interface Side (srpErrorsIntervalInterfaceSide)

Interface side containing this row information.

### Interface Number (srpErrorsIntervalNumber)

A number between 1 and 96, which identifies the interval for available statistics.

1 means interval is the most recent completed 15 minute interval.

N means interval precedes N-1.

## Related Topics

The CiscoView Monitor Window

Monitoring Ports

Monitoring the Device

Monitoring the Device Environment

Monitoring Devices and Components