# RP Registration Denied Statistics

This dialog box displays Packet Control Function (PCF) and Service Option (SO)-based RP Registration Denied Statistics.

## Navigation

1. Right-click the device, and select Monitor.

2. Select CDMA PDSN PCF & SO Based Statistics from the Category list.

3. Select a row and click the RP Registration Statistics button.

4. Select RP Registration Denied Statistics from the Category list.

The following information appears:

> Registration Requests Denied (cCdmaPcfSoRpRegDeniedReqs)

> Registration Requests Discarded (cCdmaPcfSoRpRegDiscardedReqs)

> New Connection Requests Denied (cCdmaPcfSoRpInitRegDeniedReqs)

> Re-registration Requests Denied (cCdmaPcfSoRpReRegDeniedReqs)

> De-registration Requests Denied (cCdmaPcfSoRpDeRegDeniedReqs)

> Handoff A11 Reg Req Denied (cCdmaPcfSoRpHandoffRegDeniedReqs)

### Registration Requests Denied (cCdmaPcfSoRpRegDeniedReqs)

The number of A11 registration requests denied since system startup.

### Registration Requests Discarded (cCdmaPcfSoRpRegDiscardedReqs)

The number of A11 registration requests silently discarded since system startup.

### New Connection Requests Denied (cCdmaPcfSoRpInitRegDeniedReqs)

Since system startup, the number of denied A11 registration requests meant for establishing new R-P connections.

### Re-registration Requests Denied (cCdmaPcfSoRpReRegDeniedReqs)

The number of denied A11 registration requests meant for refreshing the established R-P connections since system startup.

### De-registration Requests Denied (cCdmaPcfSoRpDeRegDeniedReqs)

The number of denied A11 registration requests meant for de-establishing the established R-P connections since system startup.

### Handoff A11 Reg Req Denied (cCdmaPcfSoRpHandoffRegDeniedReqs)

The total number of denied handoff A11 registration requests meant for already existing session, since system startup.