# CDMA PDSN Session Table

The table displays following information:

Mobile Station ID (cCdmaSessionMsid)

MSID Type (cCdmaSessionMsidType)

Electronic Serial Number (cCdmaSessionEsn)

Serving PDSN IpAddress (cCdmaSessionPdsnIp)

FA PDSN IpAddress (cCdmaSessionFaIp)

MoIP HA IpAddress (cCdmaSessionA11HaIp)

MoIP FAIpAddress (cCdmaSessionA11FaIp)

Session Key (cCdmaSessionKey)

Connection ID (cCdmaSessionConnId)

MoMt Indicator (cCdmaSessionMoMtInd)

PPP Compress Enable (cCdmaSessionPppCompressEnabled)

VJ Compress Enable (cCdmaSessionVJCompressEnabled)

Service Option (cCdmaSessionServiceOption)

Session Start Time (cCdmaSessionConnStartTime)

### Mobile Station ID (cCdmaSessionMsid)

Identifier for a mobile station.

### MSID Type (cCdmaSessionMsidType)

Format of a Mobile station ID.

'imsi' | IMSI format ( 15 digits max.)
'min' | MIN format ( 10 digits max. )
'irm' | IRM format ( 10 digits max.)
other | other formats.

### Electronic Serial Number (cCdmaSessionEsn)

Electronic serial number of a mobile station.

### Serving PDSN IpAddress (cCdmaSessionPdsnIp)

IP address of serving packet data serving node.

### FA PDSN IpAddress (cCdmaSessionFaIp)

PDSN IP address serving as foreign agent to mobile station.

### MoIP HA IpAddress (cCdmaSessionA11HaIp)

Mobile IP home agent address on A11 interface.

### MoIP FAIpAddress (cCdmaSessionA11FaIp)

Mobile IP foreign agent address on A11 interface.

### Session Key (cCdmaSessionKey)

Session identification key used by GRE protocol.

### Connection ID (cCdmaSessionConnId)

Connection ID of IP/GRE sesssion. Consists of four octets locally unique within a PDSN session.

### MoMt Indicator (cCdmaSessionMoMtInd)

Mobile originated/Mobile terminated indicator.

Values area:

other (1) |
mobileOriginated(2) | Mobile station initiated the session.
mobileTerminated (3) | Packet Data Serving Node intitiated the session.

### PPP Compress Enable (cCdmaSessionPppCompressEnabled)

PPP compression status.

Values are:

true | PPP compression is enabled.
false | PPP compression is not enabled.

### VJ Compress Enable (cCdmaSessionVJCompressEnabled)

Van-Jacobson compression status of TCP/IP header.

Values are:

true | Van-Jacobson compression is enabled.
fales | Van-Jacobson compression is not enabled.

### Service Option (cCdmaSessionServiceOption)

Type of data service and rate set used.

### Session Start Time (cCdmaSessionConnStartTime)

Session starting date and time, as provided by RAN. Agent only propogates this information.