# SSG Port Maps

The SSG Port Maps category of the Configure dialog box displays details on the service selection gateway (SSG) port map.

## Procedure

1. Right-click the device, then select Configure, or double-click the device.

2. Select SSG Port Maps from the Category list.

The following information appears:

Port Map Address Type (cssgPortMapSourceIpType)

Port Map Address (cssgPortMapSourceIp)

Lower Port Range (cssgPortMapPortRangeFrom)

Upper Port Range (cssgPortMapPortRangeTo)

Port Map RowStatus (cssgPortMapRowStatus)

### Port Map Address Type (cssgPortMapSourceIpType)

Value that represents the type of IP address stored in cssgPortMapSourceIP object.

### Port Map Address (cssgPortMapSourceIp)

Service selection gateway (SSG) source IP addresses to be used while translating the network addresses of downstream traffic (traffic from subscriber to SSG).

### Lower Port Range (cssgPortMapPortRangeFrom)

Lower limit of the range of ports in port map.

### Upper Port Range (cssgPortMapPortRangeTo)

Upper limit of the range of ports in port map.

### Port Map RowStatus (cssgPortMapRowStatus)

Status of the table entry.

Status can be used to create or delete conceptual rows in the table.

To create a row, set the object to createAndGo. cssgPortMapPortRangeFrom and cssgPortMapPortRangeTo are mandatory objects for a create request.

To delete a row, set the object to destroy.