# TACACS+

Device>Configure>TACACS+

Use the TACACS+ dialog box to set Terminal Access Controller Access Control System (TACACS+) parameters for the device.

Login Authentication (tacacsLoginAuthentication)

Whether TACACS+ login authentication is enabled on the device.

Local Login Authentication (tacacsLocalLoginAuthentication)

Whether login authentication using a local password is enabled on the device.

Enable Authentication (tacacsEnableAuthentication)

Whether TACACS+ enable authentication is enabled on the device.

Local Enable Authentication (tacacsLocalEnableAuthentication)

Whether enable authentication using a local password is enabled on the device.

Allowed Login Attempts (tacacsNumLoginAttempts)

Number of login attempts allowed on the device. Valid values are 1 to 10.

Direct Request (tacacsDirectedRequest)

Whether the TACACS+ directed request feature is enabled on the device.

Time Out (tacacsTimeout)

Number of seconds the device waits for a response from the TACACS+ server host.

Authentication Key (tacacsAuthKey)

Key used to encrypt the data passed between the TACACS+ server and this client. This key must match the one configured on the server. You must have Read/Write access to the device to change this value.

Click Apply to make your changes to these eight values take effect.

TACACS+ Server's IP (tacacsServerAddr)

IP address of this TACACS+ server.

TACACS+ Server Type (tacacsServerType)

Type of this TACACS+ server: primary or other.

Click Add to add a new entry to this table, or click Delete to remove the selected entry. Click Primary to make the selected entry the primary server.

Click Cancel to close the dialog box without making any changes. Click Print to print the contents of the dialog box.