# Mobile Router Interface Statistics

## Navigation

1. Right-click the device, and select Configure. The Device Configuration dialog box appears.

2. Select Mobile Router Interface Configs from the Category list.

3. Select a row and click the Monitor button.

The following information appears:

> Current Retransmission (cmiMrIfSolicitRetransRemaining)

> No of Retransmissions (cmiMrIfSolicitRetransCount)

> Time Remaining (cmiMrIfCCoaRegRetryRemaining)

### Current Retransmission (cmiMrIfSolicitRetransRemaining)

The time remaining before the current retransmission interval expires.

### No of Retransmissions (cmiMrIfSolicitRetransCount)

The number of retransmissions of the solicitation.

### Time Remaining (cmiMrIfCCoaRegRetryRemaining)

The time remaining before the current CCoA registration retry interval expires.