# Console, Auxiliary, and TTY Port Configuration Information

The following configuration and session information is displayed for a console, auxiliary, or TTY port:

Active

Type

Autobaud

Input Speed

Output Speed

Flow Control

Modem Control

Location

Terminal Type

Idle Timeout

Sessions in Use

TACACS User Name

# Active (tsLineActive)

Indicates whether the specified line is active or not.

# Type (tsLineType)

Indicates the type of line for which the information is displayed. The line type is one of the following:

Unknown

Console

Terminal

Line-printer

Virtual-terminal

Auxiliary

# Autobaud (tsLineAutobaud)

Indicates whether the line is set to autobaud detection so that it can adapt to the rate at which data is being sent to it. Possible values are:

1 | autobaud
0 | no autobaud

# Input Speed (tsLineSpeedin)

Indicates the line speed at which the line is running.

# Output Speed (tsLineSpeedout)

Indicates the output speed at which the line is running.

# Flow Control (tsLineFlow)

Indicates the type of flow control that the line is using. The flow can be controlled from software or hardware. The input value indicates that the flow control is coming from the device to the terminal service. The output value indicates that flow control is provided by the terminal service.

Possible values are

unknown

none

software-input

software-output

software-both

hardware-input

hardware-output

hardware-both

# Location (tsLineLoc)

Describes the physical location of the line.

# Terminal Type (Line)

Describes the terminal type of the line.

# Idle Timeout (tsLineSestmo)

Specifies the interval (in seconds) for closing the connection when there is no input or output traffic during a session.

# Sessions in Use (tsLineNses)

Indicates the number of current sessions on the line.

# TACACS User Name (tsLineUser)

Displays the Terminal Access Controller Access System (TACACS) username. TACACS servers provide security for accessing terminals remotely.