# Number of Cold Starts

## Navigation

1. Right-click the device and then select Configure > Redundant Framework > History.

2. With an entry in the history table selected, click Monitor.

This dialog box displays the following information:

### Cold Starts (cRFHistoryColdStarts)

Indicates the number of system cold starts. This value includes the number of system cold starts due to switchover failure and the number of manual restarts.