# CDMA PDSN Handoff Statistics

This dialog box is applicable to Member and Peer to Peer clusters. It displays the handoff statistics for the packet data serving node (PDSN).

## Navigation

1. Right-click the Multiprocessor WAN Application Module (MWAM), then select Configure > MWAM module.

2. With a device selected in the MWAM module table, click Statistics.

3. Select CDMA PDSN Handoff Statistics.

The following information is displayed:

> Inter PCF Handoffs (cCdmaInterPcfHandoffs)

> Inter PDSN Handoffs (cCdmaInterPdsnHandoffs)

> CANID/PANID change Handoffs (cCdmaIdChangeHandoffs)

### Inter PCF Handoffs (cCdmaInterPcfHandoffs)

Total number of inter packet control function (PCF) handoffs since the system last restarted.

### Inter PDSN Handoffs (cCdmaInterPdsnHandoffs)

Total number of inter PDSN handoffs since the system last restarted.

### CANID/PANID change Handoffs (cCdmaIdChangeHandoffs)

Total number of handoffs, because of current access network identifier/previous access network identifier (CANID/PANID) changes, since the system last restarted.