# VMPS

The following VLAN Membership Policy Server (VMPS) options are available:

Client

Sets VLAN Membership Policy Server (VMPS) parameters for this device.

Server

Sets parameters for downloading software from a VMPS.

VMPS Server MAC-to-VLAN

Displays the mapping of port MAC addresses to VLANs on this device.

Client: VQP

Displays VQP information for the device.

# Client

Device>Configure>VMPS

The Client dialog box lets you set VLAN Membership Policy Server (VMPS) parameters for this device.

Last Accessed VMPS (vmpsAccessed)

IP address of the last VMPS server accessed from this device.

Last VMPS Action (vmpsAction)

Last action requested from the VMPS server.

VMPS Address (vmpsAddr)

IP address of this VMPS server.

VMPS Type (vmpsType)

Type of this VMPS server: primary or other.

Click Reconfirm to reconfirm all dynamic VLAN assignments on the device. Click OK to continue. Click Apply to save the changes in the dialog box. Click Cancel to close the dialog box. Click Create to add a new entry to this table. Click Delete to remove the selected entry. Click Refresh to update the contents of the dialog box. Click Print to print the contents of the dialog box. Click Help to access online help.

# Server

Device>Configure>VMPS>Server

The Server dialog box lets you set parameters for downloading software from a VLAN Membership Policy Server (VMPS).

Operational Status (vmpsOperStatus)

Current status of the VMPS server: active or inactive.

Administrative Status (vmpsAdminStatus)

Desired status of the VMPS server: active or inactive. To change the status, change this value and click Modify.

Last VMPS Restart (vmpsLastRestart)

Length of time since the VMPS server was last restarted.

Total Requests Received (vmpsInConfigReqs)

Number of configuration requests received by this VMPS server.

Invalid Requests Received (vmpsInConfigErrors)

Number of configuration errors received by this VMPS server.

Rejected Responses Sent (vmpsOutConfigFails)

Number of failed configurations sent by this VMPS server

Last Rejected Client's MAC (vmpsLastFailClient)

MAC address of the last client rejected by this VMPS server.

Configuration Server's IP (vmpsDownloadServerAddress)

IP address of the host supplying TFTP configuration data for the VMPS.

Configuration File Name (vmpsConfigFileName)

Filename of the configuration file downloaded by the VMPS.

Click Download to initiate a TFTP download of the configuration file. Click OK to continue. Click Cancel to close the dialog box. Click Print to print the contents of the dialog box. Click Help to access online help.

# VMPS Server MAC-to-VLAN

Device>Configure>VMPS Server MAC-to-VLAN

The VMPS Server MAC-to-VLAN dialog box displays the mapping of port MAC addresses to VLANs on this device.

VMPS MAC (vmpsMacConfigAddress)

MAC address of this station.

VLAN Name (vmpsMacConfigVlan)

Name of VLAN associated with this MAC address.

Last Accessed (vmpsMacConfigLastAccessed)

Last time this entry was used to map a MAC address to a VLAN.

Last Requested (vmpsMacConfigLastRequestor)

IP address of the device that last requested the VLAN associated with this MAC address.

Requested Port ID (vmpsMacConfigLastRequestPortID)

ID of the port included in this configuration request.

Last Response Status (vmpsMacConfigLastResponseStatus)

Response received for this configuration request: success, versionNotSupported, insufficientResources, accessDenied, postShutdown, or unknownManagementDomain.

Click OK to continue. Click Apply to save the changes in the dialog box. Click Cancel to close the dialog box. Click Refresh to update the contents of the dialog box. Click Print to print the contents of the dialog box. Click Help to access online help.

# Client: VQP

Device>Configure>VMPS>Client:VQP

The Client:VQP dialog box displays VQP information for the device.

VQP Request Count (vmVQPQueries)

Total number of VQP requests sent by this device.

VQP Response Count (vmVQPResponses)

Total number of VQP responses received by this device.

VMPS Change Count (vmVmpsChanges)

Number of times the current VMPS has changed.

VQP Shutdown Count (vmVQPShutdown)

Total number of 'shutdown' VQP responses received by this device.

VQP Denied Count (vmVQPDenied)

Total number of denied' VQP responses received by this device.

VQP Wrong Domain Count (vmVQPWrongDomain)

Total number of VQP responses indicating the wrong management domain received by this device.

VQP Wrong Version Count (vmVQPWrongVersion)

Total number of VQP responses indicating the wrong VQP version received by this device.

VQP Insufficient Resource Count (vmInsufficientResources)

Total number of VQP responses indicating insufficient resources received by this device.

VLAN Query Protocol Version (vmVmpsVQPVersion)

VQP version supported on this device.

Number of VQP Request Retries (1..10) (vmVmpsRetries)

Number of retries for VQP requests to a VMPS that should be attempted by the device before using the next available VMPS.

VQP Reconfirm Interval (0..120) (vmVmpsReconfirmInterval)

Time, in minutes, between reconfirmations of the membership addresses on the switch with VMPS. When the value of this object is zero, the switch does not reconfirm membership with VMPS.

Current VMPS Used (vmVmpsCurrent)

IP address of the VMPS currently in use.

Click OK to continue. Click Apply to save the changes in the dialog box. Click Cancel to close the dialog box. Click Refresh to update the contents of the dialog box. Click Print to print the contents of the dialog box. Click Help to access online help.