# Virtual Switch Overview

Virtual switch functionality enables a network administrator to take two switches from the local distribution layer and combine them virtually so that they can be managed from one point/IP address. The virtual switch will look and act as a single device to both the wiring closet and the core layer.

After the wiring closet switch recognizes the two connected switches as a single device, it can create a port bundle to the virtual switch. This simplifies management because the wiring closet switch only has to deal with the lone virtual port (the uplink bundle) connected to the virtual switch.

## Related Topics

> Virtual Switch Navigation

> Hardware and Software Requirements for Virtual Switch Support

> Virtual Switch LED Legend