# Frame Relay - DLC

The table displays the frame relay data link connection information.

## Procedure

1. Right-click on the serial port and select Configure from the popup menu or double-click on the serial port. The port configuration table appears.

2. Select Frame Relay - DLC from the Category drop-down list box.

Dialog box displays following information:

> State (frDlcmiState)

> Address (frDlcmiAddress)

> Address Length (frDlcmiAddressLen)

> Status Enq Msg Intervals (frDlcmiPollingInterval)

> Max Errs Enq Status Msg (frDlcmiErrorThreshold)

> Multicast Service (frDlcmiMulticast)

> Max Virtual Circuits (frDlcmiMaxSupportedVCs)

> Monitored Events (frDlcmiMonitoredEvents)