# GTP Path History Table

## Navigation

1. Right-click the Multi-processor WAN Application Module (MWAM) and then select Configure, or double-click the module.
2. Select MWAM module from the Category drop-down box.
3. With a device selected in the MWAM module dialog box, click Statistics.
4. Select GTP Path History Table from the Category drop-down box.

The following information appears:

> Index (cGtpHistIndex)

> Remote Address Type (cGtpHistRemoteAddrType)

> Remote Address (cGtpHistRemoteAddress)

> Remote Port Number (cGtpHistRemotePort)

### Index (cGtpHistIndex)

History number of an entry.

### Remote Address Type (cGtpHistRemoteAddrType)

Internet address type value for cGtpHistRemoteAddress.

### Remote Address (cGtpHistRemoteAddress)

Internet address for the remote end of a GPRS Tunneling Protocol (GTP) path, such as the address of the serving GPRS support node (SGSN).

### Remote Port Number (cGtpHistRemotePort)

Port number for the remote end of a GTP path.