# Router Card Configure

The following options are available for configuring a router card:

Chassis

System Software

Configuration Files

Flash Memory

IP Table

Configuration Status

Configuration History

VLAN Interface Table

PCMCIA Flash Memory Display

TTY/Console Port Display

# Chassis

Configure>Chassis, Configure>Chassis

The Chassis dialog box displays general hardware configuration information for the router module.

ROM Monitor Version (romVersion)

ROM monitor version for the router.

ROM System Version (romSysVersion)

ROM system version for the router.

Memory (processorRam)

Amount of RAM, in bytes, available to the router CPU.

Configuration Memory (nvRAMSize)

Amount of non-volatile configuration memory, in bytes, installed in the router.

Configuration Memory in Use (nvRAMUsed)

Amount of non-volatile configuration memory, in bytes, currently in use.

Configuration Register (configRegister)

Current value of the configuration register.

Click Cancel to close the dialog box. Click Print to print the contents of the dialog box.

# System Software

Configure>System Software, Configure>System Software

The System Software dialog box lists the name of the system boot image and the reason it was last loaded.

IOS Name (sysConfigName)

Name of the system boot image.

Reason of Last Reload (whyReload)

Reason why the system was last restarted.

Click Cancel to close the dialog box. Click Print to print the contents of the dialog box.

# Configuration File

Configure>Configuration File, Configure>Configuration File

The Configuration File dialog box displays software and host information for the router.

Network Config Boot Address (netConfigAddr)

IP address of the host that supplied the network configuration file for the router.

Network Config Filename (netConfigName)

Name of the network configuration file.

Host Config Boot Address (hostConfigAddr)

IP address of the host that supplied the host configuration file for the router.

Host Config Filename (hostConfigName)

Name of the host configuration file.

Click Cancel to close the dialog box. Click Print to print the contents of the dialog box.

# Flash Memory

Configure>Flash Memory, Configure>Flash Memory

The Flash Memory dialog box shows the size and space available for each defined flash partition on the module.

Type (ciscoFlashPartitionName)

Name identifying this flash partition. This name can have up to 16 characters.

Memory (ciscoFlashPartitionSize)

Size of this flash partition, in bytes.

Memory Free (ciscoFlashPartitionFreeSpace)

Space available in this flash partition, in bytes.

Click Cancel to close the dialog box. Click Print to print the contents of the dialog box.

# IP Table

Configure>IP Table, Configure>IP Table

The IP Table dialog box lists network addressing information for the module.

Port (ipAdEntIfIndex)

Unique interface value for this entry.

IP Address (ipAdEntAddr)

IP address for this entry.

Subnet Mask (ipAdEntNetMask)

Subnet mask associated with this IP address.

Broadcast Format (ipAdEntBcastAddr)

Value of the least significant bit in the broadcast address used by this entry.

Reasm MaxSize (ipAdEntReasmMaxSize)

The size of the largest IP datagram which this entity can reassemble from incoming IP fragmented datagrams received on this interface.

Click Cancel to close the dialog box. Click Print to print the contents of the dialog box.

# Configuration Status

Configure>Configuration Status, Configure>Configuration Status

The Configuration Status dialog box lists current configuration information for the module.

Running Last Changed (ccmHistoryRunningLastChanged)

The date and time when the running configuration was last changed. If this value is greater than the Running Last Saved value, the configuration has been changed but not saved.

Running Last Saved (ccmHistoryRunningLastSaved)

The date and time when the running configuration was last saved (written).

Startup Last Changed (ccmHistoryStartupLastChanged)

The date and time when the startup configuration was last written to. In general, this is the default configuration used when cold starting the system. It could have been changed by a save of the running configuration or by a copy from elsewhere.

Maximum Event Entries (ccmHistoryMaxEventEntries)

The maximum number of entries that can be held in the History Event Table. The recommended value for implementations is 10.

Entries Bumped (ccmHistoryEventEntriesBumped)

The number of times the oldest entry in the History Event Table was deleted to make room for a new entry.

Click Cancel to close the dialog box. Click Print to print the contents of the dialog box.

# Configuration History

Configure>VR>Configuration History, Configure>VR>Configuration History

The Configuration History dialog box lists configuration events that have affected the module.

Event Time (ccmHistoryEventTime)

The date and time when the event occurred.

Command Source (ccmHistoryEventCommandSource)

The source of the command that initiated the event.

Config Source (ccmHistoryEventConfigSource)

The configuration data source for the event.

Config Destination (ccmHistoryEventConfigDestination)

The configuration data destination for the event.

Terminal Type (ccmHistoryEventTerminalType)

If the Command Source value is 'commandLine', this is the terminal type.

Terminal Number (ccmHistoryEventTerminalNumber)

If the Command Source value is 'commandLine', this is the terminal number. The value is -1 if the number is not available or not applicable.

Terminal User (ccmHistoryEventTerminalUser)

If the Command Source value is 'commandLine', this is the name of the logged in user. The value is zero if the name is not available or not applicable.

Terminal Location (ccmHistoryEventTerminalLocation)

If the Command Source value is 'commandLine', this is the hard-wired location of the terminal or the remote host for an incoming connection. The value is zero if the location is not available or not applicable.

Command Source Address (ccmHistoryEventCommandSourceAddress)

If the Terminal Type value is 'virtual', this is the internet address of the connected system. If the Command Source value is 'snmp', this is the internet address of the requester. The value is 0.0.0.0 if the address is not available or not applicable.

Virtual Host Name (ccmHistoryEventVirtualHostName)

If the Terminal Type value is 'virtual', this is the host name of the connected system. The value is zero if the host name is not available or not applicable.

Server Address (ccmHistoryEventServerAddress)

If the Config Source or Config Destination value is 'networkTftp' or 'networkRcp', this is the internet address of the storage file server. The value is 0.0.0.0 if the address is not applicable or not available.

Config File (ccmHistoryEventFile)

If the Config Source or Config Destination value is 'networkTftp' or 'networkRcp', this is the configuration file name at the storage file server. The value is zero if the file name is not available or not applicable.

Remote Copy (rcp) User (ccmHistoryEventRcpUser)

If the Config Source or Config Destination value is 'networkRcp', this is the remote user name. The length is zero if the user name is not applicable or not available.

Click Cancel to close the dialog box. Click Print to print the contents of the dialog box.

# VLAN Interface Table

Configure>VLAN Interface Table, Configure>VLAN Interface Table

The VLAN Interface Table dialog box lists the logical VLAN interfaces defined on the router module.

Description (ifDescr)

Text description of the logical VLAN interface.

Last Change (ifLastChange)

Date and time of the last change to the operational status of the logical VLAN interface.

In Octets (ifInOctets)

Number of octets of data received on the logical VLAN interface.

Out Octets (ifOutOctets)

Number of octets of data transmitted on the logical VLAN interface.

Click Cancel to close the dialog box. Click Print to print the contents of the dialog box.

# PCMCIA Flash Memory Display

Configure>VR>PCMCIA Flash Memory Display

The PCMCIA Flash Memory Display dialog box lists the defined flash files.

File Name (ciscoFlashFIleName)

Flash file name. Specify this name when copying the file.

File Status (ciscoFlashFIleStatus)

Status of the flash file: valid, invalid (bad checksum), or deleted.

File Size (ciscoFlashFIleSize)

Size of the flash file in bytes, including the file header

Click Cancel to close the dialog box. Click Print to print the contents of the dialog box.

# TTY/Console Port Display

Configure>RCON

The TTY/Console Port Display dialog box displays configuration information for the TTY or Console port on the module.

Active (tsLineActive)

Whether the specified line is active.

Type (tsLineType)

Type of line: console, terminal, line-printer, virtual-terminal, auxiliary, or unknown

Autobaud (tsLineAutobaud)

Whether the line is set to autobaud detection so that it can adapt to the rate at which data is being sent to it.

Input Speed (tsLineSpeedIn)

Line speed at which the line is running.

Output Speed (tsLineSpeedOut)

Output speed at which the line is running.

Flow Control (tsLineFlow)

Type of flow control that the line is using. The flow can be controlled from software or hardware. The input value indicates that the flow control is coming from the device to the terminal service. The output value indicates that flow control is provided by the terminal service.

Modem Control (tsLineModem)

type of modem control the line is using. Possible values include: Call-in, Call-out, Cts-required Ri-is-cd, and Inout.

Location (tsLineLoc)

Physical location of the line.

Terminal Type (tsLineTerm)

Terminal type of the line.

Idle Timeout (tsLineTmo)

Interval (in seconds) for closing the connection when there is no input or output traffic during a session.

Session In Use (tsLineNses)

Number of current sessions on the line.

TACACS User Name (tsLineUser)

Terminal Access Controller Access System (TACACS) username. TACACS servers provide security for accessing terminals remotely.

Click Cancel to close the dialog box. Click Print to print the contents of the dialog box.