# CDMA PDSN Registration Denied Stats

This dialog box is applicable to Controller, Member, and Peer to Peer clusters. From here, you can view registration statistics for denied requests.

## Navigation

1. Right-click the Multiprocessor WAN Application Module (MWAM), then select Configure > MWAM module.

2. With a device selected in the MWAM module table, click Statistics.

3. Select CDMA PDSN Registration Denied Stats.

The following data is displayed:

> Registration Request Denied (cCdmaRpRegDeniedReqs)

> Registration Request Discarded (cCdmaRpRegDiscardedReqs)

> Registration Request for New connection Denied (cCdmaRpInitRegDeniedReqs)

> Registration Request for Refreshing connection Denied (cCdmaRpReRegDeniedReqs)

> Registration Request for Disconnection Denied (cCdmaRpDeRegDeniedReqs)

### Registration Request for Disconnection Denied (cCdmaRpDeRegDeniedReqs)

Number of denied A-11 registration requests since system startup that are used for deactivating the established R-P connections.

The code field in the registration reply is set to non-zero.

### Registration Request Denied (cCdmaRpRegDeniedReqs)

Number of A-11 registration requests denied since system startup.

The code field in the registration reply is set to non-zero.

### Registration Request Discarded (cCdmaRpRegDiscardedReqs)

Number of A-11 registration requests discarded since system startup.

A registration reply is not returned for these A-11 registration requests.

### Registration Request for New connection Denied (cCdmaRpInitRegDeniedReqs)

Number of denied A-11 registration requests since system startup that are used for establishing new R-P connections. These A-11 registration requests contain the connection setup airlink record.

The code field in the registration reply is set to non-zero.

### Registration Request for Refreshing connection Denied (cCdmaRpReRegDeniedReqs)

Number of denied A-11 registration requests since system startup that are used for refreshing the established R-P connections.

The code field in the registration reply is set to non-zero.