# Basic Info

Configure>Repeater>Basic Info

To show basic information for the selected repeater, select Basic Info from the CATEGORY popup menu in the CiscoView Configure Repeater window.

The CiscoView Configure Repeater window shows the following information:

Group Capacity (rptrGroupCapacity)

Number of groups that can be contained within the repeater.

Oper Status (rptrOperStatus)

Operational state of the repeater: ok, rptrFailure, groupFailure, portFailure, generalFailure, or other.

Health (rptrHealthText)

Information about the general health of the repeater. The information is agent-specific.

Number of Partitioned Ports (rptrTotalPartitionedPorts)

Total number of auto-partitioned ports on this repeater.

Reset (rptrReset)

Setting this value to reset will reset the repeater.

Non Disrupt Test (rptrNonDisruptTest)

Setting this value to selfTest causes the repeater to perform an agent-specific non-disruptive self test. This test does not interfere with data transfer or other management functions.