# Displaying QLLC Link Station Statistics

To display QLLC link station statistics in the CiscoView Configure window, select QLLC from the CATEGORY popup menu. The following information is displayed:

Circuit Type (qllcLSOperCircuit Type)

Operation Role (qllcLSOperRole)

Remote X.25 Addr (qllcLSOperX25Add)

Operation State (qllcLSOperState)

Modulus (qllcLSOperModulo)

Largest Packet Out (qllcLSOperLgX25)

# Circuit Type (qllcLSOperCircuit Type)

Indicates whether the circuit type on the interface is switchedVC (switched virtual circuit) or permanentVC (permanent virtual circuit).

# Operation Role (qllcLSOperRole)

Indicates the role of the specified QLLC link station. Possible values are primary, secondary, and peerToPeer.

# Remote X.25 Addr (qllcLSOperX25Add)

Displays the remote X.25 address associated with the QLLC connection.

# Operation State (qllcLSOperState)

Indicates the state of a particular QLLC connection as defined in the IBM document “The X.25 1984/1988 DTE/DCE and DTE/DTE Interface Architecture Reference,” document number SC30-3409-1.

# Modulus (qllcLSOperModulo)

Indicates the modulus for the QLLC link station. Possible values are modulo8 and modulo128.

# Largest Packet Out (qllcLSOperLgX25)

Indicates the largest QLLC packet allowed to go out on the QLLC/X.25 side.