# Fast Serial Port Configuration Information

The following information is displayed for a fast serial port:

> Type (locIfFSIPtype)

> RTS Signal (locIFSIPrts)

> CTS Signal (locIFSIPcts)

> DTR Signal (locIFSIPdtr)

> DCD Signal (locIFSIPdcd)

> DSR Signal (locIFSIPdsr)

Type (locIfFSIPtype)

Indicates whether the FSIP line uses data communications equipment (DCE) or data terminal equipment (DTE).

RTS Signal (locIfFSIPrts)

Indicates whether the RTS (request to send) signal is up or down. Possible values are up, down, and not available.

CTS Signal (locIfFSIPcts)

Indicates whether the CTS (clear to send) signal is up or down. Possible values are up, down, and not available.

DTR Signal (locIfFSIPdtr)

Indicates whether the DTR (data terminal ready) signal is up or down. Possible values are up, down, and not available.

DCD Signal (locIfFSIPdcd)

Indicates whether the DCD (data carrier detect) signal is up or down. Possible values are up, down, and not available.

DSR Signal (locIfFSIPdsr)

Indicates whether the DSR (data set ready) field is up or down. Possible values are up, down, and not available.