# MWAM Module

## Navigation

Right-click the Multiprocessor WAN Application Module (MWAM), then select Configure > MWAM module.

The following information is displayed:

> Device ID (cdpCacheDeviceId)

> Address (cdpCacheAddress)

> Device Platform (cdpCachePlatform)

> Processor Details

### Device ID (cdpCacheDeviceId)

Device identifier string, as reported in the most recent Cisco Discovery Protocol (CDP) message. A zero-length string indicates that no Device ID field (TLV) was reported.

### Address (cdpCacheAddress)

First network-layer address of the SNMP agent on the device, as reported in the most recent CDP message. For example, if the corresponding instance of cacheAddressType has the value "ip(1)", then this object is an IP address.

### Device Platform (cdpCachePlatform)

Hardware platform of the device, as reported in the most recent CDP message. A zero-length string indicates that no Platform field (TLV) was reported.

### Processor Details

Indicates the type of image running in the MWAM processor. There are eight possible values:

> Unreachable IP

> GGSN

> SSG

> PDSN Controller

> PDSN Member

> PDSN–Peer to Peer

> Home Agent

> Unknown Config