# Console, Auxiliary, and TTY Port Configuration Information

The following configuration and session information is displayed for a console, auxiliary, or TTY port:

> Active (tsLineActive)

> Type (tsLineType)

> Autobaud (tsLineAutobaud)

> Input Speed (tsLineSpeedin)

> Output Speed (tsLineSpeedout)

> Flow Control (tsLineFlow)

> Modem Control (tsLineModem)

> Location (tsLineLoc)

> Terminal Type (tsLineTerm)

> Idle Timeout(secs) (tsLineTmo)

> Sessions In Use (tsLineNses)

> TACACS User Name (tsLineUser)

Active (tsLineActive)

Indicates whether the specified line is active or not.

Type (tsLineType)

The type of line for which the information is displayed. The line type is one of the following:

Unknown

Console

Terminal

Line-printer

Virtual-terminal

Auxiliary

Autobaud (tsLineAutobaud)

Indicates whether the line is set to autobaud detection which enables it to adapt to the rate at which data is being sent to it.
Values are:

1 | autobaud
0 | no autobaud

Input Speed (tsLineSpeedin)

The line input speed at which the line is running.

Output Speed (tsLineSpeedout)

The output speed at which the line is running.

Flow Control (tsLineFlow)

The type of flow control that is being used on the line. The flow can be controlled from software or hardware. The input value indicates that the flow control is coming from the device to the terminal service. The output value indicates that flow control is provided by the terminal service.

Possible values are

Unknown

None

Software-input

Software-output

Software-both

Hardware-input

Hardware-output

Hardware-both

Location (tsLineLoc)

Describes the physical location of the line.

Terminal Type (tsLineTerm)

Describes the terminal type of the line.

Idle Timeout(secs) (tsLineTmo)

Interval (in seconds) after which the connection is closed when there is no input or output traffic during a session.

Sessions In Use (tsLineNses)

Number of current sessions on the line.

TACACS User Name (tsLineUser)

Displays the Terminal Access Controller Access Control System (TACACS) username. TACACS servers provide security for remote terminal access.

Modem Control (tsLineModem)

Modem control the line is using.

Possible values are:

unknown(1),

none(2),

call-in(3),

call-out(4),

cts-required(5),

ri-is-cd(6),

inout(7)