# GGSN Access Point Throughput Statistics

## Procedure

1. Right-click the Multi-processor WAN Application Module (MWAM), then select Configure, or double-click the module.

2. Select MWAM module from the Category list.

3. Select a row and click Statistics.

4. Select category GGSN Access Point Throughput Statistics.

The following information appears:

> Access Point Index (cgprsAccPtIndex)

> Collection Interval (cgprsAccPtThruputInterval)

### Access Point Index (cgprsAccPtIndex)

A locally unique identifier for this access point on this GGSN.

### Collection Interval (cgprsAccPtThruputInterval)

This object represents the time interval at which the statistics are sampled. Interval configuration is out

of the scope of the MIB and are covered in CISCO-GGSN-MIB.