# Switched Virtual Interface: Configure

The Configure SVI dialog box allows you to enter the details for creating a switched virtual interface (SVI). An SVI is a switch interface with an IP address that is a layer 3 LAN.

VLAN Interface ID

IP Address

Subnet Mask

Interface Status

From the SVI Configure dialog box:

To create an SVI click Create.

To modify an SVI, select a row, then click Modify.

### VLAN Interface ID

Identifier of the VLAN interface.

### IP Address

IP address of the VLAN interface.

### Subnet Mask

Mask IP address of the VLAN interface.

### Interface Status

Status of the VLAN interface. Status can be Up or Down.