# Monitoring Serial Port Information

The CiscoView Monitor Port window displays the following information for a serial port:

Aborted Pkts

Misaligned Pkts

Carrier Sig Trans

Overruns

Checksum Err Pkts

# Aborted Pkts (locIfInAbort)

Shows the number of input packets that were aborted.

# Carrier Sig Trans (locIfCarTrans)

Shows the number of times the interface detected the carrier signal transition.

# Overruns (locIfInOverrun)

Shows the amount of input that arrived too quickly for the hardware to receive.

# Checksum Err Pkts (locIfInCRC)

Shows the number of input packets that had cyclic redundancy check (CRC) errors.