# RP Registration Failures

Use this option to view Packet Control Function (PCF) and Service Option (SO) based RP Registration Failures.

## Procedure

To access RP Registration Failures information:

1. Right-click the device and select Monitor from the popup menu.

2. Select CDMA PDSN PCF & SO Based Statistics from the Category menu.

3. Select any row and click on RP Registration Statistics.

4. Select RP Registration Failures from the Category menu.

The following information appears

> Unknown Failures (cCdmaPcfSoRpRegPcfUnknwnFails)

> Administrative Failures (cCdmaPcfSoRpRegAdmnFails )

> Insufficient Resource Failures (cCdmaPcfSoRpRegNoRsrcFails)

> MN Authentication Failures (cCdmaPcfSoRpRegMNAuthFails)

> ID Mismatch Failures (cCdmaPcfSoRpRegIdMismatFails)

> Bad Request Failures (cCdmaPcfSoRpRegBadReqFails)

### Unknown Failures (cCdmaPcfSoRpRegPcfUnknwnFails)

Since system startup, the number of registration requests that failed when the Packet Control Function (PCF) address did not appear in the PDSN's list of configured PCFs for an unspecified reason.

### Administrative Failures (cCdmaPcfSoRpRegAdmnFails )

Since system startup, the number of registration requests that failed when the PCF address did not appear in the PDSN's list of configured PCFs since system startup.

### Insufficient Resource Failures (cCdmaPcfSoRpRegNoRsrcFails)

Since system startup, the number of registration requests that failed when the number of PCFs or sessions reached the maximum, or when system resources were insufficient.

### MN Authentication Failures (cCdmaPcfSoRpRegMNAuthFails)

Number of registration requests that failed due to Mobile Node (MN) authentication failure since system startup.

### ID Mismatch Failures (cCdmaPcfSoRpRegIdMismatFails)

Number of registration requests that failed due to an identification mismatch since system startup.

### Bad Request Failures (cCdmaPcfSoRpRegBadReqFails)

Number of registration requests that failed due to a badly formed request since system startup.