# RSVP RESV Message Table

Displays the information describing the state information displayed by receivers in RESV messages.

> Reservation Request Number

> Session Type

> Destination Address

> Sender Address

> Destination Address Length

> Sender Address Length

> Protocol

> Destination Port

> Source Port

> QOS Service

> Status

> Time to Live

> Flow ID

### Reservation Request Number (rsvpResvNumber)

Indicates the number of a reservation request. This is for SNMP indexing only and has no relation to any protocol value.

### Session Type (rsvpResvType)

Indicates the type of session, for example IP4, IP6, IP6 with flow information.

### Destination Address (rsvpResvDestAddr)

Indicates the destination address used by all senders in a session. The destination address may not changed when the RowStatus is active.

### Sender Address (rsvpResvSenderAddr)

Indicates the sender's source address selected by a reservation. A value of all zeroes indicates 'all senders'. Sender Address may not be changed when the RowStatus is active.

### Destination Address Length (rsvpResvDestAddrLength)

Indicates the CIDR prefix length of the destination address. The IP4 host and multicast address value is 32.

The value of this object may not be changed when the RowStatus is active.

### Sender Address Length (rsvpResvSenderAddrLength)

Indicates the CIDR prefix length of sender's address. The value is 32 for IP4 host and multicast addresses. The value of this object may not be changed when the RowStatus is active.

### Protocol (rsvpResvProtocol)

Indicates the IP Protocol used by a session. The value of this object may not be changed when the RowStatus is active.

### Destination Port (rsvpResvDestPort)

Indicates the UDP or TCP port number used as a destination port for all senders in a session.

If the IP Protocol in use, specified by rsvpResvProtocol, is 50 (ESP) or 51 (AH), this represents a virtual desination port number. Zero indicates that the IP protocol in use does not have ports.

The value of this object may not be changed when the RowStatus is active.

### Source port (rsvpResvPort)

Indicates the UDP or TCP port number used as a source port for the sender in a session. If the IP protocol in use, specified by rsvpResvProtocol is 50(ESP) or 51 (AH), this represents a generalized port identifier (GPI). Zero indicates that the IP protocol in use does not have ports. This object may not be changed when the value of the RowStatus is active.

### QoS Service (rsvpResvService)

Indicates the QoS Service classification requested by the receiver.

### Status (rsvpResvStatus)

Indicates the status of RESV messages. Displays active for active RESV messages.

The value may be used to install static RESV information or delete RESV information.

### Time to Live (rsvpResvTTL)

Indicates the TTL value in the last received RSVP header.

### Flow ID (rsvpResvFlowId)

Indicates the flow ID a receiver is using in an Ipv6 session.