# RSVP Resv Forward Table

Specifies the state of information displayed upstream in RESV messages.

Table displays the following information:

Session Number

Session Type

Destination Address

Sender Address

Destination Address Length

Sender Address Length

Protocol

Destination Port

Sender Port

QoS Service

Status

Time to Live

Flow ID

### Session Number (rsvpResvFwdNumber)

Displays the number of reservation request.

Note: This is for SNMP indexing only and has no relation to any protocol value.

### Session Type (rsvpResvFwdType)

Specifies the type of session (IP4, IP6, etc.).

### Destination Address (rsvpResvFwdDestAddr)

Indicates the destination address used by all senders in a session. The value should not be changed when the value of the RowStatus is active.

### Sender Address (rsvpResvFwdSenderAddr)

Specifies the source address of the sender selected by a reservation.

A value of all zeroes indicates all senders. The sender address may not be changed when the value of the RowStatus is active.

### Destination Address Length (rsvpResvFwdDestAddrLength)

Indicates the length of the destination address in bits. The value should not be changed when the value of the RowStatus is active.

### Sender Address Length (rsvpResvFwdSenderAddrLength)

Inidicates the length of the sender's address in bits. The value should not be changed when the value of the RowStatus is active.

### Protocol (rsvpResvFwdProtocol)

Specifies the IP protocol used by a session. For secure sessions Protocol indicates IP security. The value should not be changed when the value of the RowStatus is active.

### Destination Port (rsvpResvFwdDestPort)

Indicates the UDP or TCP port number used as a destination port for all senders for the specified session. If the protocol in use, specified by rsvpResvFwdProtocol, is 50 (ESP) or 51 (AH), this represents a virtual destination port number. If the value is zero, the IP protocol in use does not have ports.

The value of this object may not be changed when the value of the RowStatus object is active.

### Sender Port (rsvpResvFwdPort)

Indicates the UDP or TCP port number used as a source port for a sender in a session. IP protocol in use, specified by rsvpResvFwdProtocol is 50 (ESP) or 51 (AH), this represents a generalized port identifier (GPI). If the value is zero, the IP protocol in use does not have ports.

The value of this object may not be changed when the value of the RowStatus object is active.

### QoS Service (rsvpResvFwdService)

Indicates the QoS service Classification requested.

### Status (rsvpResvFwdStatus)

Indicates the status of the RESV messages. Displays active for all active messages. Status information may be used to delete RESV information.

### Time to Live (rsvpResvFwdTTL)

Indicates the TTL value in the last received RSVP header.

### Flow ID (rsvpResvFwdFlowId)

Indicates the flow ID used by the receiver in an IPv6 session.