# Token Ring Port Configuration Information

The Token Ring Port Configuration window displays the following information:

Index

Command

Error Report

Open/Close Info

Result of Last Enter Ring

Speed

Upstream Neighbor MAC Address

# Index (dot5IfIndex)

Specifies the ifIndex value from the MIB interface table for this interface.

# Command (dot5Commands)

Specifies the name of a command variable used to request a state change. Possible values are no-op, open, reset, or close.

Open means join the ring; close means leave.

# Error Report (dot5RingStatus)

Displays the number of errors on the specified port.

# Open/Close Info (dot5RingStatus)

Provides information related to entering/leaving the ring.

# Result of Last Enter Ring (dot5RingOpenStatus)

Indicates if the last attempt to enter the ring was successful, and if not, shows the reason for the failure.

# Speed (dot5RingSpeed)

Indicates the bandwidth for the ring. Possible values are 1 Mbps, 4 Mbps, 16 Mbps, or unknown. A read-only variable.

# Upstream Neighbor MAC Address (dot5RingUpStream)

Specifies the MAC address of the upstream neighbor.