# Power Over Ethernet Details

## Navigation

Power over Ethernet Module > Config > Power Over Ethernet Details

This dialog box provides the power details for a Power over Ethernet module.

The following information is displayed:

> Nominal Power (pethMainPsePower)

> Total Used Power (pethMainPseConsumptionPower)

> Inline Power Status (pethMainPseOperStatus)

> Threshold Notification (pethNotificationControlEnable)

> Threshold Value (pethMainPseUsageThreshold)

### Nominal Power (pethMainPsePower)

Nominal power of the main power source entity (PSE), measured in watts.

### Total Used Power (pethMainPseConsumptionPower)

Total amount of power used by the main PSE, measured in watts.

### Inline Power Status (pethMainPseOperStatus)

Operational status of the main PSE.

### Threshold Notification (pethNotificationControlEnable)

When the value of this object is true, it indicates that agent notifications are enabled.

### Threshold Value (pethMainPseUsageThreshold)

When the PSE exceeds the power usage percentage specified by this object, an alarm is generated.