# Circuits

The following circuit information is displayed:

Status

Time Call Send/Recvd

Direction of Call

# Status (x25CircuitStatus)

Specifies the current status of the specified circuit.

# Time Call Send/Recvd (x25CircuitEstablishTime)

Specifies the value of the sysUpTime MIB descriptor when the channel was associated with this circuit.

# Direction of Call (x25CircuitDirection)

Specifies the direction of the call that established this circuit. Possible values are incoming, outgoing, or pvc.