# CDMA PDSN A11 Registration Statistics

## Navigation

1. Right-click the device, and select Monitor. The Monitor Device dialog box appears.
2. Select CDMA PDSN A11 Registration Statistics from the Category list.

The following information appears:

> Accepted A11 for De-established R-P Conn (cCdmaRpDeRegHandoffAcceptedReqs)

> Initial A11 Registration Req (cCdmaRpInitRegReceivedReqs)

> A11 Re- Registration Req (cCdmaRpReRegReceivedReqs)

> A11 De-Registration Req (cCdmaRpDeRegReceivedReqs)

> Handoff A11 Registration Req (cCdmaRpHandoffRegReceivedReqs)

> Accepted Handoff A11 Registration Req (cCdmaRpHandoffRegAcceptedReqs)

> Airlink Start A11 Registration Reg (cCdmaRpReRegAirlinkStarts)

> Airlink Stop A11 Registration Reg (cCdmaRpReRegAirlinkStops)

> Airlink Stop A11 De-Registration Reg (cCdmaRpDeRegAirlinkStops)

### Accepted A11 for De-established R-P Conn (cCdmaRpDeRegHandoffAcceptedReqs)

The total number of accepted A11 Registration Requests meant for de-establishing the already established R-P connections with the Packet Control Function (PCF) from which the mobile node was handed off since the system was last restarted. The Code field in the corresponding Registration Reply message is set to zero.

### Initial A11 Registration Req (cCdmaRpInitRegReceivedReqs)

The number of Initial A11 Registration Requests received since the system was last restarted.

### A11 Re- Registration Req (cCdmaRpReRegReceivedReqs)

The number of A11 Re-Registration Requests received since the system was last restarted.

### A11 De-Registration Req (cCdmaRpDeRegReceivedReqs)

The number of A11 De-Registration Requests received since the system was last restarted.

### Handoff A11 Registration Req (cCdmaRpHandoffRegReceivedReqs)

The number of A11 Handoff Registration Requests received since the system was last restarted.

### Accepted Handoff A11 Registration Req (cCdmaRpHandoffRegAcceptedReqs)

The total number of accepted handoff A11 Registration Requests meant for the already existing session, since the system was last restarted.

### Airlink Start A11 Registration Reg (cCdmaRpReRegAirlinkStarts)

The number of A11 Re-Registration Requests containing Airlink Start since the system was last restarted.

### Airlink Stop A11 Registration Reg (cCdmaRpReRegAirlinkStops)

The number of A11 Re-Registration Requests containing Airlink Stop since the system was last restarted.

### Airlink Stop A11 De-Registration Reg (cCdmaRpDeRegAirlinkStops)

The number of A11 De-Registration Requests containing Airlink Stop since the system was last restarted.