# CSG Quota Manager Statistics2

## Navigation

1. Right-click the Service and Application Module for IP (SAMI) card and then select Configure.
2. Select SAMI module from the Category drop-down box.
3. With a device selected, click Statistics.
4. Select Content Services Gateway from the Category drop-down box.
5. Select CSG Quota Server from the Category drop-down box.
6. With a table entry selected, click Monitor.
7. Select CSG Quota Manager Statistics2 from the Category drop-down box.

The following information appears:

> Messages to be ACKed (ccsQuotaMgrOutstanding)

> Time to Reset HighWater (ccsQuotaMgrHighWaterResetTime)

> Bad Records Received (ccsQuotaMgrBadRecord)

> Max Bad Records Received (ccsQuotaMgrHCBadRecord)

> Messages Retransmitted (ccsQuotaMgrRetransmit)

> Max Messages Retransmitted (ccsQuotaMgrHCRetransmit)

### Messages to be ACKed (ccsQuotaMgrOutstanding)

Current number of messages waiting to be acknowledged.

### Time to Reset HighWater (ccsQuotaMgrHighWaterResetTime)

Indicates when ccsgsUserHighWater was last reset to zero.

### Bad Records Received (ccsQuotaMgrBadRecord)

Number of bad records received. These are records in which an error was detected while attempting to decode its contents.

### Max Bad Records Received (ccsQuotaMgrHCBadRecord)

Number of bad records received. These are records in which an error was detected while attempting to decode its contents.

This object is a 64-bit version of ccsQuotaMgrBadRecord.

### Messages Retransmitted (ccsQuotaMgrRetransmit)

Number of messages retransmitted to the quota manager.

### Max Messages Retransmitted (ccsQuotaMgrHCRetransmit)

Number of messages retransmitted to the quota manager.

This object is a 64-bit version of ccsQuotaMgrRetransmit.