# Device Tracking Details

## Navigation

Device > Configure > EOU > IP Device Tracking

The following information appears:

> Tracking Enabled (cnnIpDeviceTrackingEnabled)

> Tracking Probe Count (cnnIpDeviceTrackingProbeCount)

> Tracking Probe Interval (cnnIpDeviceTrackingProbeInterval)

### Tracking Enabled (cnnIpDeviceTrackingEnabled)

Indicates whether the IP device tracking feature is globally enabled on this device.

### Tracking Probe Count (cnnIpDeviceTrackingProbeCount)

The number of times this device sends the ARP probe to an IP device before removing that device from the IP device tracking table.

### Tracking Probe Interval (cnnIpDeviceTrackingProbeInterval)

The number of seconds this device waits before resending the ARP probe.