# Mobile Router Registration Configs

## Navigation

1. Right-click the device, and select Configure. The Device Configuration dialog box appears.

2. Select category Mobile Router Registration Configs from the Category list.

The following information appears:

> Time before Lifetime Expiration (cmiMrRegExtendExpire)

> Number of Retries (cmiMrRegExtendRetry)

> Waiting Time for Reply (cmiMrRegExtendInterval)

> Requested Registration Time (cmiMrRegLifetime)

> Initial Retransmission (cmiMrRegRetransInitial)

> Maximum Retransmission Time (cmiMrRegRetransMax)

> Max Retransmissions (cmiMrRegRetransLimit)

### Time before Lifetime Expiration (cmiMrRegExtendExpire)

The time remaining in seconds to send a registration request before lifetime expiration.

### Number of Retries (cmiMrRegExtendRetry)

The number of retries to be sent.

### Waiting Time for Reply (cmiMrRegExtendInterval)

The time in seconds after which the mobile router is to send another registration request when no reply is received.

### Requested Registration Time (cmiMrRegLifetime)

The requested lifetime in seconds in registration requests.

### Initial Retransmission (cmiMrRegRetransInitial)

The time in milliseconds to wait after no reply is received before retransmitting for the first time.

### Maximum Retransmission Time (cmiMrRegRetransMax)

The maximum retransmission time allowed (milliseconds).

### Max Retransmissions (cmiMrRegRetransLimit)

The maximum number of retransmissions allowed.