# Private VLAN

Port>Configure>PrivateVLAN

The Private VLAN window contains the following MIBs:

Multi Primary VLANs (cpvlanPromPortMultiPrimaryVlan)

Indicates whether all the bits set as secondary VLANs in the corresponding remapping objects (i.e. cpvlanPromPortSecondaryRemap, cpvlanPromPortSecondaryRemap2k, cpvlanPromPortSecondaryRemap3k, cpvlanPromPortSecondaryRemap4k) can or cannot belong to multiple primary VLANs for this port.

Secondary Remap (cpvlanPromPortSecondaryRemap(1-4)k)

Secondary Remap field is a combination of the following 3 fields: cpvlanPromPortSecondaryRemap2k, cpvlanPromPortSecondaryRemap3k, cpvlanPromPortSecondaryRemap4k.

> Secondary Remap 2k (cpvlanPromPortSecondaryRemap2k)

> A string of octets containing one bit per VLAN for VLANs with VlanIndexOrZero values of 1024 through 2047 in the management domain on this port.

> Secondary Remap 3k (cpvlanPromPortSecondaryRemap3k)

> A string of octets containing one bit per VLAN for VLANs with VlanIndexOrZero values of 2048 through 3071 in the management domain on this port.

> Secondary Remap 4k (cpvlanPromPortSecondaryRemap4k)

> A string of octets containing one bit per VLAN for VLANs with VlanIndexOrZero values of 3072 through 4095 in the management domain on this port.

TwoWayCommunity Remap Capable (cpvlanPromPortTwoWayRemapCapable)

Indicates whether the port is currently in promiscuous mode for Private VLAN feature.

Note: Extended range VLAN values (1025-4094) are supported by Catalyst 4000 devices running Catalyst OS version 7.2 or later and Catalyst 6000 devices running Catalyst OS version 6.1 or later.

Click OK to continue. Click Apply to save the changes in the dialog box. Click Cancel to close the dialog box. Click Refresh to update the contents of the dialog box. Click Print to print the contents of the dialog box. Click Help to access online help.