# SRP Higher Layer Interval Statistics - History

Use this option to monitor higher layer interval statistics of an interface side with a specific interval number.

## Procedure

To access higher layer interval statistics - history information:

> 1. Right-click the SRP interface and select Configure from the popup menu.

> > The Configure Port dialog box appears.

> 2. Select SRP Higher Layer Interval Statistics - History from the Category menu.

> > SRP Higher Layer Interval Statistics - History dialog box displays:

> > Interface Side (srpHostIntInterfaceSide)

> > Interval Number (srpHostIntNumber)

3. Select an Interval to view error statistics history for that particular interval.

## Related Topics

The CiscoView Monitor Window

Monitoring Ports

Monitoring the Device

Monitoring the Device Environment

Monitoring Devices and Components

Interface Side (srpHostIntInterfaceSide)

Interface side containing this row information.

Interval Number (srpHostIntNumber)

A number between 1 and 96, which identifies an interval with available statistics.

1 means interval is the most recent completed 15 minute interval.

N means interval precedes N-1.