# Mobile Network Configs

1. Right-click on the MWAM Card and select Configure.

2. Select category MWAM module.

3. Select a row and click the Configure button.

4. Select category Mobile Network Configs.

The following information appears:

> Mobile Network Interfaces Index (cmiMrMobNetIfIndex)

> Inet Address (cmiMrMobNetAddr)

> Prefix Length Associated (cmiMrMobNetPfxLen)

> Mobile Network Address Type (cmiMrMobNetAddrType)

> Create/Delete Row (cmiMrMobNetStatus)

> Tunnel Interfaces Index (cmiMrHaTunnelIfIndex)

##

### Mobile Network Interfaces Index (cmiMrMobNetIfIndex)

The ifIndex value from Interfaces table of MIB II for the interface on the mobile router connected to the mobile network.

### Inet Address (cmiMrMobNetAddr)

IP address of the mobile network.

### Mobile Network Address Type (cmiMrMobNetPfxLen)

Prefix length associated with the mobile network IP address.

### Mobile Network Address Type (cmiMrMobNetAddrType)

Type of IP address stored in cmiMrMobNetAddr.

### Create/Delete Row (cmiMrMobNetStatus)

Row status for the mobile network entry.

### Tunnel Interfaces Index (cmiMrHaTunnelIfIndex)

The ifIndex value from Interfaces table of MIB II for the tunnel interface (to HA) of the mobile router.