# X.25 Port Statistics

## Procedure

> 1. Right-click on the port and select Monitor from the popup menu. The port monitor dialog box appears.

> 2. Select X.25 Port statistics from the drop-down list box.

The CiscoView Monitor Port dialog box displays the following performance information for an X.25 port:

> In Interrupts (x25CircuitInInterrupts)

> Out Interrupts (x25CircuitOutInterrupts)

> In Octets (x25CircuitInOctets)

> Out Octets (x25CircuitOutOctets)

> Data RTx Timeouts (x25CircuitDataRetransmissionTimeouts)

> Reset Timeouts (x25CircuitResetTimeouts)

> Interrupt Timeouts (x25CircuitInterruptTimeouts)

In Interrupts (x25CircuitInInterrupts)

Displays the number of interrupt packets received.

Out Interrupts (x25CircuitOutInterrupts)

Number of interrupt packets sent.

In Octets (x25CircuitInOctets)

Number of octets of user data delivered to the upper layer.

Out Octets (x25CircuitOutOctets)

Number of octets of user data sent.

Data RTx Timeouts (x25 CircuitDataRetransmissionTimeouts)

Number of times the T25 data retransmission timer expired.

Reset Timeouts (x25CircuitResetTimeouts)

Number of times the T22 reset timer expired.

Interrupt Timeouts (x25CircuitInterruptTimeouts)

Number of times the T26 Interrupt timer expired.