# Billing Mediation Agent Table

## Navigation

1. Right-click the Service and Application Module for IP (SAMI) card and then select Configure.
2. Select SAMI module from the Category drop-down box.
3. With a device selected, click Statistics.
4. Select Content Services Gateway from the Category drop-down box.
5. Select Billing Agent from the Category drop-down box.

The following information appears:

> VRF Name (ccsBMAVrfName)

> IP Address Type (ccsBMAIpAddrType)

> IP Address (ccsBMAIpAddr)

> Port No (ccsBMAPort)

> State (ccsBMAState)

### VRF Name (ccsBMAVrfName)

Name of the VPN routing/forwarding (VRF) instance over which communication with the billing mediation agent (BMA) occurs. If no VRF instance is specified, then the global routing table is used.

### IP Address Type (ccsBMAIpAddrType)

Indicates the address type of ccsBMAIpAddr.

### IP Address (ccsBMAIpAddr)

IP address of a BMA.

### Port No (ccsBMAPort)

UDP port configured for a BMA.

### State (ccsBMAState)

Status of a BMA. There are six possible values:

> standby—The BMA is ready to become active.

> failed—The BMA has failed to respond to requests.

> active—The BMA is ready to receive requests.

> echowait—An echo request has been sent to this BMA and is waiting for a response.

> nawait—A node-alive request has been sent to this BMA and is waiting for a response.

> suspended—The BMA has received a stop request from the operator.