# High Priority Traffic

Use this option to monitor statistics of high priority traffic transmission to physical medium-dependent layer for current interval for a particular side of a particular SRP interface.

## Procedure

To access monitor high priority traffic information:

1. Right-click the port and select SRP Interface Statistics from the pop-up menu.

Media Dependent Current Interval Statistics dialog box appears.

2. Select Tx Physical Layer Statistics from the Category menu to display transmission physical layer statistics information.

3. Select High Priority Traffic from the Category menu to display high priority traffic information.

High Priority Traffic dialog box displays:

Unicast High Priority Packets (SrpRingCurUcastHighPriPktsOut)

Unicast High Priority Octets (SrpRingCurUcastHighPriOctetsOut)

Multicast High Priority Packets (SrpRingCurMcastHighPriPktsOut)

Multicast High Priority Octets (SrpRingCurMcastHighPriOctetsOut)

### Unicast High Priority Packets (SrpRingCurUcastHighPriPktsOut)

Number of high-priority unicast packets going to the physical medium-dependent layer during a 15-minute interval.

### Unicast High Priority Octets (SrpRingCurUcastHighPriOctetsOut)

Number of high-priority unicast octets going to the physical medium-dependent layer during a 15-minute interval.

### Multicast High Priority Packets (SrpRingCurMcastHighPriPktsOut)

Number of high-priority multicast packets going to the physical medium-dependent layer during a 15-minute interval.

### Multicast High Priority Octets (SrpRingCurMcastHighPriOctetsOut)

Number of high-priority multicast octets going to the physical medium-dependent layer during a 15-minute interval.

## Related Topics

Using CiscoView Interface

Using the Main Menu

Selecting Components

Configuring Devices and Components

Monitoring Devices and Components