# Home Agent Registration Statistics2

## Navigation

1. Right-click the Multiprocessor WAN Application Module (MWAM), then select Configure > MWAM module.

2. With a device selected in the MWAM module table, click Statistics.

3. Select Home Agent Registration Statistics2.

The following information is displayed:

> Poorly Formed Requests (haPoorlyFormedRequest)

> Innumerous Mobility Bindings ( haTooManyBindings)

> HA Address Unknown (haUnknownHA)

> Gratuition ARPs Sent (haGratuitiousARPsSent)

> Proxy ARPs Sent (haProxyARPsSent)

> Registration Replies Ratio (haRegRepliesSent/haRegRequestsReceived)

> Deregistration Replies Ratio (haDeRegRepliesSent/haDeRegRequestsReceived)

### Poorly Formed Requests (haPoorlyFormedRequest)

Total number of registration requests denied by the home agent—poorly formed request (code 134).

### Innumerous Mobility Bindings (haTooManyBindings)

Total number of registration requests denied by the home agent—too many simultaneous mobility bindings (code 135).

### HA Address Unknown (haUnknownHA)

Total number of registration requests denied by the home agent—unknown home agent address (code 136).

### Gratuition ARPs Sent (haGratuitiousARPsSent)

Total number of gratuition ARPs sent by the home agent on behalf of mobile nodes.

### Proxy ARPs Sent (haProxyARPsSent)

Total number of proxy ARPs sent by the home agent on behalf of mobile nodes.

### Registration Replies Ratio (haRegRepliesSent/haRegRequestsReceived)

> haRegRepliesSent: Total number of registration replies sent by the home agent.

> haRegRequestsReceived: Total number of registration requests received by the home agent.

### Deregistration Replies Ratio (haDeRegRepliesSent/haDeRegRequestsReceived)

> haDeRegRepliesSent: Total number of registration replies sent by the home agent in response to deregistration requests.

> haDeRegRequestsReceived): Total number of registration requests received by the home agent with a lifetime of zero (requests to deregister).