# CDMA PDSN System Information

From this dialog box, you can view Packet Data Serving Node (PDSN) system information.

## Navigation

1. Right-click the Mobile Wireless Application Module (MWAM), then select Configure > MWAM module.

2. With a device selected in the MWAM module table, click Configure.

3. Select CDMA PDSN System Information.

The following information is displayed:

> Max Number of Sessions (cCdmaSessionMaxAllowed)

> Max Number of PCF (cCdmaPcfMaxAllowed)

> Host Name (cCdmaServingPdsnHostname)

> PDSN System Version (cCdmaSystemVersion)

> PDSN Authentication Timer (cCdmaSessionPdsnAuthenTimer)

> Max Session Notification Enable (cCdmaSessionMaxNotifEnabled)

> Max PCF Notification Enable (cCdmaPcfMaxAllowedNotifEnabled)

> Invalid Registration Notification Enable (cCdmaRegReqFailedNotifEnabled)

> PDSN Status (cCdmaSystemStatus)

> Session Low Threshold Allowed (cCdmaSessionLowThreshold)

> Session High Threshold Allowed (cCdmaSessionHighThreshold)

> Session Redundancy Enabled (cCdmaSrEnabled)

### Max Number of Sessions (cCdmaSessionMaxAllowed)

Maximum number of sessions allowed by the system. This object is applicable to member and peer-peer.

When the value of this object is zero, there are no limitations on the number of PDSN sessions.

### Max Number of PCF (cCdmaPcfMaxAllowed)

Maximum number of packet control functions (PCF) allowed by system. This object is applicable to member and peer-peer.

When the value of this object is zero, there are no limitations on the number of PCF sessions.

### Host Name (cCdmaServingPdsnHostname)

Host name of the serving PDSN. This object is applicable to controller, member and peer-peer.

### PDSN System Version (cCdmaSystemVersion)

Cisco packet data switching node release version (for example, output: 1.1). This object is applicable to controller, member and peer-peer.

### PDSN Authentication Timer (cCdmaSessionPdsnAuthenTimer)

Timer for Mobile IP (MoIP) users not using PPP authentication. This object is applicable to member and peer-peer.

### Max Session Notification Enable (cCdmaSessionMaxNotifEnabled)

When the value of this object is true, a notification is sent when the maximum number of sessions is reached. This object is applicable to member and peer-peer.

Note: The default value is false.

### Max PCF Notification Enable (cCdmaPcfMaxAllowedNotifEnabled)

When the value of this object is true, a notification is sent when the maximum number of interconnected PCF are reached. This object is applicable to member and peer-peer.

Note: The default value is false.

### Invalid Registration Notification Enable (cCdmaRegReqFailedNotifEnabled)

When the value of this object is true, a failure notification is sent to the manager whenever a session terminates because of a registration request failure. When enabled, this object is applicable to controller, member and peer-peer.

Note: The default value is false.

### PDSN Status (cCdmaSystemStatus)

Operational status of the PDSN subsystem. This object is applicable to controller, member and peer-peer.

### Session Low Threshold Allowed (cCdmaSessionLowThreshold)

Minimum number of allowed sessions. The agent generates a notification when this threshold is reached during call release. This object is applicable to member and peer-peer.

### Session High Threshold Allowed (cCdmaSessionHighThreshold)

Maximum number of allowed sessions. The agent generates a notification when this threshold is reached during call setup. This object is applicable to member and peer-peer.

### Session Redundancy Enabled (cCdmaSrEnabled)

Indicates whether the session redundancy feature is enabled.

Note: This object is available only in PSDN 2.0.