# CDMA PDSN Inter PCF Handoff Registration Update Statistics

Use this option to view Inter Packet Control Function (PCF) Handoff Registration Update Statistics.

## Procedure

To access CDMA PDSN Inter PCF Handoff Registration Update Statistics information:

1. Right-click the device and select Monitor from the popup menu.

2. Select CDMA PDSN Inter PCF Handoff Registration Update Statistics from the Category menu.

The following information appears:

> Updates by PCF Handoffs (cCdmaRpUpdPcfHandoffs)

> Updates Not Acknowledged (cCdmaRpUpdHandoffNotAckedReqs)

> Updates Acknowledged (cCdmaRpUpdHandoffReceivedAcks)

> Updates Accepted (cCdmaRpUpdHandoffAcceptedReqs)

> Updates Denied (cCdmaRpUpdHandoffDeniedReqs)

> Registration Acknowledgements Discarded (cCdmaRpUpdHandoffDiscardedAcks)

> Initial Updates Sent(cCdmaRpUpdHandoffInitTxdReqs)

> Retransmitted Updates (cCdmaRpUpdHandoffReTxdReqs)

> Note: All these statistics are a result of inter PCF handoffs.

### Updates by PCF Handoffs (cCdmaRpUpdPcfHandoffs)

Number of updated registrations sent as a result of inter PCF handoffs since system startup.

### Updates Not Acknowledged (cCdmaRpUpdHandoffNotAckedReqs)

Number of A11 registration updates received that were unacknowledged since system startup.

### Updates Acknowledged (cCdmaRpUpdHandoffReceivedAcks)

Number of A11 registration updates received that were acknowledged since system startup.

### Updates Accepted (cCdmaRpUpdHandoffAcceptedReqs)

Number of A11 registration acknowledgements received with the Status field set to zero since system startup.

### Updates Denied (cCdmaRpUpdHandoffDeniedReqs)

Number of A11 registration acknowledgements received with the Status field set to non-zero since system startup.

### Registration Acknowledgements Discarded (cCdmaRpUpdHandoffDiscardedAcks )

Number of A11 registration acknowledgements discarded since system startup.

### Initial Updates Sent (cCdmaRpUpdHandoffInitTxdReqs)

Number of initial A11 registration updates sent as the result of inter PCF handoffs since system startup.

### Retransmitted Updates (cCdmaRpUpdHandoffReTxdReqs)

Number of A11 registration updates that were retransmitted because the initial registration update was not acknowledged or was denied since system startup.